**Maurice CE-SDS PLUS Cartridge**

|  |  |  |  |
| --- | --- | --- | --- |
| **Part Number** | 090-157 | **Serial Number** |  |
| **Product Name** | Maurice CE-SDS PLUS Cartridge | **Date of Manufacture** |  |
|  |  | **Expiration Date** |  |

This product was tested on a Maurice system and passed all physical and functional test criteria.

**Test Methods**

Analysis of Maurice CE-SDS PLUS Cartridge on Maurice or Maurice S. systems. All tests were performed using ProteinSimple’s reduced IgG standard. **Figure 1**, representative electropherogram for Reduced IgG standard, Peaks: internal standard (IS, 10KD), light chain (LC), non-glycosylated heavy chain (NGHC), glycosylated heavy chain (HC).

# **ACCEPTANCE RESULTS**

|  |  |  |
| --- | --- | --- |
| Parameter | Acceptance Criteria | Pass/Fail |
| Resolution, HC (Reduced Sample) | ≥ 1.50 | Pass |
| Peak Height, HC (Reduced Sample) | ≥ 20.0 mAU | Pass |

Reviewed and Approved:

A picture containing clipart, linedrawing

Description automatically generated

Hooi Tan

Sr. Quality Manager

Date: